**Important Notice.**

**Set-up for leaning ladders and stepladders:**

**Pre-Visual, Pre-use check.**

* **Missing, damaged or worn anti-slip feet on metal and fibreglass ladders.**
* **Items such as swarf, stones, grease, dirt etc. stuck in the feet preventing the feet from making direct contact with the ground.**
* **Mud, grease or oil either on the rungs or the stiles.**
* **Cracks in the rungs or stiles.**
* **Missing, broken or weakened rungs.**
* **Cracked or damaged welds and missing or loose screws or rivets on metal ladders.**
* **For stepladders – locking device is intact.**